Contents

# OSI and TCP Layer

Diagram

Description automatically generated

Figure - 1




Figure – 2




Figure - 3

Note : -

1. IEEE 802.3 - Ethernet

IEEE 802.11 – WiFi

1. Ethernet frame Normal IEEE 802.3 compliant Ethernet frames are between 64 and 1518 bytes long.
2. Ping: - ICMP is used for testing network connections using ping program.

In progress -- [KM, 44, 30:00]